# Mocap model issues:

## Transferring joint angles:

Files related: JointAngleOutputs.any, JointsAndDriversOptimized.any

Problems:

* Model does not load unless the files exist. This is a real problem with the combined model where both kinematics and inverse dynamics are in one model.
* Model has to be reloaded after joint angles are save to the file
* Adding new body parts or other things to the model is a pain.